|  |
| --- |
| **True / False** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1. Short pants cut off above the knee are appropriate for masons in extremely hot weather.   |  |  |  | | --- | --- | --- | |  | a. | True | |  | b. | False |  |  |  | | --- | --- | | *ANSWER:* | False | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 2. Hard hats are required only for construction jobs that have been determined to have excessive hazards.   |  |  |  | | --- | --- | --- | |  | a. | True | |  | b. | False |  |  |  | | --- | --- | | *ANSWER:* | False | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 3. Because the spray can obstruct vision, goggles are not recommended when using a wet saw.   |  |  |  | | --- | --- | --- | |  | a. | True | |  | b. | False |  |  |  | | --- | --- | | *ANSWER:* | False | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 4. If you constantly have to raise your voice to shout or be hear, the noise level is too high, and you should use ear plugs.   |  |  |  | | --- | --- | --- | |  | a. | True | |  | b. | False |  |  |  | | --- | --- | | *ANSWER:* | True | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 5. Employers must also, according to the law, conduct safety training for their employees regarding hazardous chemicals or products in the work area.   |  |  |  | | --- | --- | --- | |  | a. | True | |  | b. | False |  |  |  | | --- | --- | | *ANSWER:* | True | |

|  |
| --- |
| **Multiple Choice** |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 6. Lightweight plastic hats, commonly called \_\_\_\_\_, afford little protection and do not conform to regulations.   |  |  |  | | --- | --- | --- | |  | a. | hard hats | |  | b. | bump hats | |  | c. | plastic caps | |  | d. | hard shells |  |  |  | | --- | --- | | *ANSWER:* | b | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 7. A hard hat has two parts: the \_\_\_\_\_ and the \_\_\_\_\_ .   |  |  |  | | --- | --- | --- | |  | a. | metal; foam | |  | b. | visor; casing | |  | c. | skin; padding | |  | d. | shell; suspension materials |  |  |  | | --- | --- | | *ANSWER:* | d | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8. Hearing protection should be worn when the noise exposure level \_\_\_\_\_ .   |  |  |  | | --- | --- | --- | |  | a. | exceeds 90 decibels | |  | b. | reaches 75 decibels | |  | c. | is less than 80 decibels | |  | d. | approaches 85 decibels |  |  |  | | --- | --- | | *ANSWER:* | a | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 9. Mortar pans should be placed back from the walls approximately \_\_\_ to allow proper working space.   |  |  |  | | --- | --- | --- | |  | a. | 5' | |  | b. | 3' | |  | c. | 2' | |  | d. | 6" |  |  |  | | --- | --- | | *ANSWER:* | c | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 10. Safety nets made of \_\_\_\_\_ are stronger, lighter in weight, and more resistance to wear and weather elements than the original safety nets.   |  |  |  | | --- | --- | --- | |  | a. | manilla rope | |  | b. | chain mail | |  | c. | synthetic fibers | |  | d. | natural fibers |  |  |  | | --- | --- | | *ANSWER:* | c | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 11. Grounded electrical plugs can be easily identified because they have \_\_\_\_\_ .   |  |  |  | | --- | --- | --- | |  | a. | three prongs | |  | b. | orange cords | |  | c. | UL-tested tags | |  | d. | triangular heads |  |  |  | | --- | --- | | *ANSWER:* | a | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 12. After prolonged use, the head of a chisel becomes flared out from striking with a steel hammer, thus the chisel becomes \_\_\_\_\_ or burred.   |  |  |  | | --- | --- | --- | |  | a. | gourded | |  | b. | mashed | |  | c. | cupped | |  | d. | mushroomed |  |  |  | | --- | --- | | *ANSWER:* | d | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 13. Protective safety rod caps should be made of \_\_\_\_\_ .   |  |  |  | | --- | --- | --- | |  | a. | rigid plastic | |  | b. | thick rubber | |  | c. | cast concrete | |  | d. | flexible plastic |  |  |  | | --- | --- | | *ANSWER:* | a | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 14. \_\_\_\_\_ scaffolding can consist of one or more platforms supported by rigid, strong, load-bearing members or supports, such as tubular steel sections, poles, frames, masts, and outriggers.   |  |  |  | | --- | --- | --- | |  | a. | Suspending | |  | b. | Swinging | |  | c. | Lifting | |  | d. | Supporting |  |  |  | | --- | --- | | *ANSWER:* | d | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 15. \_\_\_\_\_ are injuries to the muscular or skeletal framework parts of the body.   |  |  |  | | --- | --- | --- | |  | a. | MSs | |  | b. | MSFs | |  | c. | WMSDs | |  | d. | WRMDs |  |  |  | | --- | --- | | *ANSWER:* | c | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 16. Which of the following statements is a good safety practice for masons?   |  |  |  | | --- | --- | --- | |  | a. | Never use gasoline-operated mortar mixers. | |  | b. | Wear rubber gloves when operating a wet masonry saw. | |  | c. | Avoid angled shields when using a saw. | |  | d. | Use lightweight household extension cords with grinders. |  |  |  | | --- | --- | | *ANSWER:* | b | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 17. Any injury serious enough to require medical attention should be reported to the supervisor or instructor \_\_\_\_\_ .   |  |  |  | | --- | --- | --- | |  | a. | immediately | |  | b. | within 24 hours of the incident | |  | c. | in written form by then end of the work/school week | |  | d. | only if transportation to a medical facility is necessary |  |  |  | | --- | --- | | *ANSWER:* | a | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 18. \_\_\_\_\_ is defined as any clothing or other equipment or devices workers wear to protect themselves from job hazards.   |  |  |  | | --- | --- | --- | |  | a. | MDSDs | |  | b. | OSHA | |  | c. | PPE | |  | d. | HAZMATs |  |  |  | | --- | --- | | *ANSWER:* | c | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 19. In the case of an emergency when no dust mask or respirator is available,  \_\_\_\_\_ will suffice until you can get out of the area.   |  |  |  | | --- | --- | --- | |  | a. | a wet handkerchief tied snugly around your face covering your mouth and nose | |  | b. | using your gloved hand to cover your mouth and nose | |  | c. | pulling your shirt up and over your mouth and nose and holding tightly with your hand | |  | d. | placing and holding your mouth and nose tightly in the bend of your elbow |  |  |  | | --- | --- | | *ANSWER:* | a | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 20. Chemical manufacturers and importers must develop or obtain a material safety data sheet for \_\_\_\_\_ .   |  |  |  | | --- | --- | --- | |  | a. | only chemicals that can burn or asphyxiate users | |  | b. | any substance that can cause a chemcial reaction | |  | c. | everything from hazardous chemicals to electrical equipment | |  | d. | each hazardous chemical they produce or distribute |  |  |  | | --- | --- | | *ANSWER:* | d | |